; Stirusb.inf
; Copyright 2000, SigmaTel, Inc.



;;++ Added by AddSDisk.cmd
[SourceDisksNames]
3426=windows cd

[SourceDisksFiles]
irstusb.sys 		= 3426
;;--

[Version]
;; Commented by AddSDisk.cmd
;; LayoutFile  = layout.inf
Signature = "$Windows NT$"
Class = Infrared
provider = %ST%
ClassGUID = {6bdd1fc5-810f-11d0-BEC7-08002BE2092F}
DriverVer=06/21/2006,6.0.6001.18000
CatalogFile.NTx86  = delta.cat

[Manufacturer]
%ST%=ST,NTx86...1

[ControlFlags]
ExcludeFromSelect = USB\VID_066F&PID_4200

[ST.NTx86...1]
%USB\VID_066F&PID_4200.DeviceDesc%=STIrUsb.Dev,USB\VID_066F&PID_4200

[DestinationDirs]
STIrUsb.CopyFiles = 12
DefaultDestDir = 12

[STIrUsb.Dev.NT]
CopyFiles=STIrUsb.CopyFiles
AddReg=STIrUsb.AddReg, STIrUsb.Params.AddReg
BusType=5
Characteristics = 0x84; NCF_PHYSICAL, NCF_HAS_UI

[STIrUsb.Dev.NT.Services]
Addservice = STIrUsb, 0x00000002, STIrUsb.AddService, common.EventLog

[STIrUsb.AddService]
DisplayName    = %STIrUsb.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\irstusb.sys
LoadOrderGroup = NDIS

[STIrUsb.AddReg]
HKR,  Ndi,            HelpText,     0,      %STIrUsb.Help%
HKR,  Ndi,            Service,      0,      "STIrUsb"
HKR,  Ndi\Interfaces, UpperRange,   0,      "ndisirda"
HKR,  Ndi\Interfaces, LowerRange,   0,      "nolower"
HKR,  Ndi,            RequiredAll,  0,      "MS_IrDA"

[STIrUsb.Params.AddReg]
HKR,Ndi\params\TransceiverType,ParamDesc,,%strRXSEL%
HKR,Ndi\params\TransceiverType,default,,"0"
HKR,Ndi\params\TransceiverType,type,,"enum"
HKR,Ndi\params\TransceiverType\enum,"0",,"SigmaTel 4012 [Default]"
HKR,Ndi\params\TransceiverType\enum,"1",,"SigmaTel 4000"
HKR,Ndi\params\TransceiverType\enum,"2",,"Vishay TFD"

;
;    IrDA Minimum Turnaround Time (value in microseconds)
;
HKR,Ndi\params\MinTurnTime,ParamDesc,,%strIRDATURNTIME%
HKR,Ndi\params\MinTurnTime,default,,"1000"
HKR,Ndi\params\MinTurnTime,type,,"enum"
HKR,Ndi\params\MinTurnTime\enum,"500",," 0.5 mS"
HKR,Ndi\params\MinTurnTime\enum,"1000",," 1.0 mS [Default]"
HKR,Ndi\params\MinTurnTime\enum,"5000",," 5.0 mS"
HKR,Ndi\params\MinTurnTime\enum,"10000",,"10.0 mS"

;
;    IrDA Speed enables
;
;
;       Note:  Miniport will always enable 9600,
;               no matter what this key says
;
HKR,Ndi\params\SpeedEnable,ParamDesc,,%strSPEEDENABLE%
HKR,Ndi\params\SpeedEnable,type,,"enum"
HKR,Ndi\params\SpeedEnable,default,,"4000000"
HKR,Ndi\params\SpeedEnable\enum,"2400",,   "   2400"
HKR,Ndi\params\SpeedEnable\enum,"9600",,   "   9600"
HKR,Ndi\params\SpeedEnable\enum,"19200",,  "  19200"
HKR,Ndi\params\SpeedEnable\enum,"38400",,  "  38400"
HKR,Ndi\params\SpeedEnable\enum,"57600",,  "  57600"
HKR,Ndi\params\SpeedEnable\enum,"115200",, " 115200" 
;HKR,Ndi\params\SpeedEnable\enum,"576000",, " 576000"
;HKR,Ndi\params\SpeedEnable\enum,"1152000",,"1152000" 
HKR,Ndi\params\SpeedEnable\enum,"4000000",,"4000000 [Default]"

[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, %SystemRoot%\System32\netevent.dll
HKR, , TypesSupported,   0x00010001, 7

[STIrUsb.CopyFiles]
irstusb.sys

;[SourceDisksFiles]
;stirusb.sys=1

;[SourceDisksNames]
;1 = %strDRIVERDISK%,,,

;---------------------------------------------------------------;

[Strings]
ST="SigmaTel, Inc."
USB\VID_066F&PID_4200.DeviceDesc="SigmaTel USB-IrDA Dongle"
STIrUsb.SvcDesc="SigmaTel USB-IrDA Dongle"
STIrUsb.Help   = "The USB-IrDA is a fast IrDA infrared port. It can be used to establish wireless serial and network links to other computers."

strRXSEL="Infrared Transceiver Type"
strIRDATURNTIME="Min. Turn-Around Time"
strSPEEDENABLE="Speed Enable"
strRXWINDOW="Receive Window"

strDRIVERDISK=""

