; Stirusb.inf
; Copyright 2000, SigmaTel, Inc.

[Version]
Signature = "$Windows NT$"
Class = Infrared
provider = %ST%
ClassGUID = {6bdd1fc5-810f-11d0-BEC7-08002BE2092F}
DriverVer = 11/03/2003,1.28.0.0 
CatalogFile = irstusb.cat

[Manufacturer]
%ST%=ST

[ControlFlags]
ExcludeFromSelect = USB\VID_066F&PID_4200

[ST]
%USB\VID_066F&PID_4200.DeviceDesc%=STIrUsb.Dev,USB\VID_066F&PID_4200

[DestinationDirs]
STIrUsb.CopyFiles = 12
DefaultDestDir = 12
                
[STIrUsb.Dev.NT]
CopyFiles=STIrUsb.CopyFiles
AddReg=STIrUsb.AddReg, STIrUsb.Params.AddReg
BusType=1
Characteristics = 0x84; NCF_PHYSICAL, NCF_HAS_UI

[STIrUsb.Dev.NT.Services]
Addservice = STIrUsb, 0x00000002, STIrUsb.AddService, common.EventLog

[STIrUsb.AddService]
DisplayName    = %STIrUsb.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\irstusb.sys
LoadOrderGroup = NDIS

[STIrUsb.AddReg]
HKR,  Ndi,            HelpText,     0,      %STIrUsb.Help%
HKR,  Ndi,            Service,      0,      "STIrUsb"
HKR,  Ndi\Interfaces, UpperRange,   0,      "ndisirda"
HKR,  Ndi\Interfaces, LowerRange,   0,      "nolower"
HKR,  Ndi,            RequiredAll,  0,      "MS_IrDA"

[STIrUsb.Params.AddReg]
;
;    Receive Mode.
;    0 = Slow - RXSLOW only (4115)
;    1 = SlowFast - both lines (HP style)
;    2 = Fast - !RXSLOW
;
HKR,,ReceiveMode,0,"2"

;
;    Transceiver Type.
;    Sets default Dpll and Sensitivity values.
;    HP setting also forces "Slow/Fast" ReceiveMode.
;
HKR,Ndi\params\TransceiverType,ParamDesc,,%strRXSEL%
HKR,Ndi\params\TransceiverType,default,,"1"
HKR,Ndi\params\TransceiverType,type,,"enum"
HKR,Ndi\params\TransceiverType\enum,"0",,"SigmaTel 4012"
HKR,Ndi\params\TransceiverType\enum,"1",,"Vishay 6101E [Default]"
HKR,Ndi\params\TransceiverType\enum,"2",,"Vishay 6102F"
HKR,Ndi\params\TransceiverType\enum,"3",,"Vishay 6102F (alternate)"
HKR,Ndi\params\TransceiverType\enum,"4",,"Infineon"
HKR,Ndi\params\TransceiverType\enum,"5",,"HP 1100"
HKR,Ndi\params\TransceiverType\enum,"6",,"Zilog ZHX2010"

;
;    IrDA Minimum Turnaround Time (value in microseconds)
;
HKR,Ndi\params\MinTurnTime,ParamDesc,,%strIRDATURNTIME%
HKR,Ndi\params\MinTurnTime,default,,"1000"
HKR,Ndi\params\MinTurnTime,type,,"enum"
HKR,Ndi\params\MinTurnTime\enum,"500",," 0.5 mS"
HKR,Ndi\params\MinTurnTime\enum,"1000",," 1.0 mS [Default]"
HKR,Ndi\params\MinTurnTime\enum,"5000",," 5.0 mS"
HKR,Ndi\params\MinTurnTime\enum,"10000",,"10.0 mS"

;
;    IrDA Speed enables
;
;
;       Note:  Miniport will always enable 9600,
;               no matter what this key says
;
HKR,Ndi\params\SpeedEnable,ParamDesc,,%strSPEEDENABLE%
HKR,Ndi\params\SpeedEnable,type,,"enum"
HKR,Ndi\params\SpeedEnable,default,,"4000000"
HKR,Ndi\params\SpeedEnable\enum,"2400",,   "   2400"
HKR,Ndi\params\SpeedEnable\enum,"9600",,   "   9600"
HKR,Ndi\params\SpeedEnable\enum,"19200",,  "  19200"
HKR,Ndi\params\SpeedEnable\enum,"38400",,  "  38400"
HKR,Ndi\params\SpeedEnable\enum,"57600",,  "  57600"
HKR,Ndi\params\SpeedEnable\enum,"115200",, " 115200" 
HKR,Ndi\params\SpeedEnable\enum,"4000000",,"4000000 [Default]"

[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

[STIrUsb.CopyFiles]
irstusb.sys

[SourceDisksFiles]
irstusb.sys=1

[SourceDisksNames]
1 = %strDRIVERDISK%,,,

;---------------------------------------------------------------;

[Strings]
ST=""
USB\VID_066F&PID_4200.DeviceDesc="ACTiSYS ACT-IR2000UL USB-IrDA Adapter"
STIrUsb.SvcDesc="STIrUsb.sys ACTiSYS ACT-IR2000UL USB-IrDA Adapter"
STIrUsb.Help   = "The ACT-IR2000UL is a fast IrDA infrared port. It can be used to establish wireless serial and network links to other computers."

strRXSEL="Infrared Transceiver Type"
strIRDATURNTIME="Min. Turn-Around Time"
strSPEEDENABLE="Speed Enable"
strRXWINDOW="Receive Window"

strDRIVERDISK="ACT-IR2000UL Install"